### Manual Rules

Window for the rules used in interactive routing when the route mode in the Route Parameter window is set to manual.

#### via rule

> In this combo box you can choose the via rule which you want to use currently in interactive routing.

#### trace clearance class:

> Use this combo box for selecting the clearance class which you want to use currently in interactive routing for traces.

#### trace width:

> Here you can edit the trace width you want to use currently in interactive routing.

#### on layer:

> Defines the layers, for which the trace width in the field above is valid. If all is selected in the combo box, the value in the trace width field is valid on all layers. If inner is selected, it is valid on all inner layers. Otherwise the value is valid only on the layer with the selected name in the combo box. The trace width field remains empty, if the trace width is layer dependent and all is selected in the combo box. Analog if inner is selected.

back