Short intro:

Paste Long Coding from VAG-COM into 1) for the ECU's available [01] [09] [19] [46]
[Tabulator] to 2) Load the right XPL file.
[Tabulator] to 3) to go through the bytes (you can also use [PgUp][PgDn]).
[Tabulator] and [Space] to change the Bit.
5) Press [Copy new Coding] if you want to use the changed Long Coding in VAG-COM.
Now you can Paste the changed Long Coding into VAG-COM.
You can also use [Arrow Down/Up] instead of [Tabulator].

You can also insert Short Coding now, fx. 131313 from Audi A6 (4F) Module [46].
See text explanation in "Balloon help" under VAG-COM Coding,
or choose the car you have at Openobd.org, fx Audi A6 (4F) Module [46] go to:
http://de.openobd.org/audi/a6_4f.htm#46
From ver. 510.0 you can also load some sxp information files for help.
From ver. 510.3 LCode can be started from VAG-COM automatic,
Long Code is automatic transfered to LCode and right XPL file is loaded.

Press [ESC] to Quit the program.

----------------------------------------------------------------------------------

In exchange for this freeware program, please send your 00 Auto-Scan values to me:
Fill in form at: http://www.netech.dk/fr-teche.html [VAG-ECU]

The latest information for long coding is available at:
http://de.openobd.org

----------------------------------------------------------------------------------

Please send corrections and new long coding explanations to:
nez@netech.dk or sebastian@openobd.org

27 February 2006