### Snapshots

In the Snapshot window the current interactive situation of the IDE can be saved for restoring it later on.

#### Description of the buttons:

> Goto Selected Snapshot

> > Restores the interactive situation, when the selected snapshot was saved. You can also double click a snapshot in the list instead.

> > To avoid frequent changing between the main window and the Snapshots window, you can use the j-key instead. With the h-key you can select the previous snapshot and with the k-key the next snapshot.

> Create

> > Here you can store current interactive situation after changing the predefined name.

> Remove Selected Snapshot

> > Removes the selected snapshot from the list.

> Remove All Snapshots

> > Removes all snapshots from the list.

> Snapshot Settings

> > Opens a window with the Snapshot Settings. There you can deselect attributes, which you do not want to be saved in a snapshot.

#### Description of the fields in the Snapshot Settings window:

> object colors

> > The current color settings of the object types will be saved in the snapshots.

> object visibility

> > The current color intensity of the single object types will be saved.

> layer visibility

> > The current intensity for displaying objects on the individual layers is saved.

> display region

> > The currently displayed region of the board will be saved.

> interactive state

> > In the snapshots will be saved, if the IDE is currently in the Select- Route- or Drag-State.

> selection layers

> > In the snapshots will be saved, if in the Select Parameter window selection layers is set to all visible or to current only.

> selectable items

> > The settings for the Selectable Items in the Select Parameter window will be saved in the snapshots.

> current layer

> > The Current Layer in the Select Parameter window will be saved.

> rule selection

> > In the snapshots will be saved, if in the Route Parameter Window the rule selection is set to automatic or to manual.

> manual rule settings

> > The settings in the Manual Rules window will be saved.

> push&shove enabled

> > In the snapshots will be saved, if in the Route Parameter push&shove enabled is selected.

> drag components enabled

> > In the snapshots will be saved, if in the Route Parameter drag components enabled is selected.

> pull tight region

> > The value for the pull tight region in the Route Parameter window will be saved.

> component grid

> > The value for the component grid in the Move Parameter window will be saved.

> info list selections

> > The selected indices and the filter strings in the windows for Incompletes, Library Packages, Library Padstacks, Placed Components and Nets will be saved.