
**** 07/29/08 23:26:13 ******* PSpice 10.1.0 (Jan 2003) ******* ID# 1111111111 
 ** Profile: "Example-book"  [ O:\AAAAAAAAAAAAAAAAAAA\Workarea\cnam C3\1\example-pspicefiles\example\book.sim ] 


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "book.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Profile Libraries :
* Local Libraries :
.INC "F:/Workarea/cnam C3/differentiel_1/models.mod" 
* From [PSPICE NETLIST] section of D:\Cadence\PSD_15.1\tools\PSpice\PSpice.ini file:

*Analysis directives: 
-----------------------------------------------------$
ERROR -- Unable to open file
.AC LIN 100 100 1Meg
.PROBE V(*) I(*) W(*) D(*) NOISE(*) 
.INC "..\Example.net" 



**** INCLUDING Example.net ****
* source EXAMPLE
M_M16         N112115 A B VM25 MODN  
+ L=1.6u  
+ W=100u         
C_CC         N112115 N111663  5pF  
M_M1         N111901 0 N111987 VP25 MODP  
+ L=1.6u  
+ W=300u         
M_M4         B N111901 VM25 VM25 MODN  
+ L=1.6u  
+ W=150u         
M_M3         N111901 N111901 VM25 VM25 MODN  
+ L=1.6u  
+ W=150u         
M_M6         N111663 C VP25 VP25 MODP  
+ L=1.6u  
+ W=300u         
M_M13         N111177 N111177 VM25 VM25 MODN  
+ L=1.6u  
+ W=25u         
M_M8         OUT N111663 VP25 VP25 MODP  
+ L=1.6u  
+ W=500u         
M_M15         N111180 N111177 N1111750 VM25 MODN  
+ L=1.6u  
+ W=100u         
M_M9         OUT B VM25 VM25 MODN  
+ L=1.6u  
+ W=500u         
M_M7         N111663 B VM25 VM25 MODN  
+ L=1.6u  
+ W=300u         
M_M2         B N115151 N111987 VP25 MODP  
+ L=1.6u  
+ W=300u         
V_VG         N91433 0 5V
V_V1_01         VDD_01 0 5V
M_M2_01         N91433 N91417 0 0 MODN  
+ L=150u  
+ W=5u         
R_R1_01         N91417 VDD_01  380k  
R_R         VM25 N1111750  8k  
M_M1_01         N91417 N91417 0 0 MODN  
+ L=150u  
+ W=5u         
M_M5         N111987 C VP25 VP25 MODP  
+ L=1.6u  
+ W=300u         
V_V3         N115151 0 DC 0Vdc AC 10mVac 
M_M10         C C VP25 VP25 MODP  
+ L=1.6u  
+ W=25u         
M_M11         A C VP25 VP25 MODP  
+ L=1.6u  
+ W=25u         
M_M14         C A N111180 VM25 MODN  
+ L=1.6u  
+ W=25u         
M_M12         A A N111177 VM25 MODN  
+ L=1.6u  
+ W=25u         
V_VPLUS         VP25 0 2.5V
V_VMOINS         0 VM25 2.5V

**** RESUMING book.cir ****
.END
