** Profile: "SCHEMATIC1-PROFILE2"  [ D:\Ancien_D\PATRICE\Travaux\C3\cnam\reference\1\ref-pspicefiles\schematic1\profile2.sim ] 

** Creating circuit file "PROFILE2.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Profile Libraries :
* Local Libraries :
.INC "D:/Ancien_D/PATRICE/Travaux/C3/cnam/reference/models.mod" 
* From [PSPICE NETLIST] section of D:\Cadence\PSD_15.1\tools\PSpice\PSpice.ini file:
.lib "D:\PSD_Data\Etage differentiel\models.mod" 
.lib "nom.lib" 

*Analysis directives: 
.DC LIN V_V1 8 11 0.1 
.TEMP -30 0 30 60 90
.INC "..\SCHEMATIC1.net" 


.END
